The binaries in this package have been tuned for different systems.

http://www.numberworld.org/y-cruncher/internals/arch-optimizations.html


--------------------------------------------------------------------------------

Binary: "19-ZN2 ~ Kagari" (AMD Zen 2)


Required Instructions:
    x64, ABM, BMI1, BMI2, ADX,
    SSE, SSE2, SSE3, SSSE3, SSE4.1, SSE4.2,
    AVX, FMA3, AVX2


Target Systems:
    - AMD Zen 2 Matisse

Recommended For:
    - AMD Zen 2 Matisse


This binary was tuned on:

    Processor(s)    :   AMD Ryzen 9 3950X
    Frequency       :   variable (stock)
    Memory          :   128 GB DDR4 @ 3200 MHz (16-18-18-38)

    Cores           :   16
    Threads         :   32
    Cache           :   64 MB
    Cache / Threads :   2 MB / thread


--------------------------------------------------------------------------------

Binary: "18-CNL ~ Shinoa" (Intel Cannon Lake)


Required Instructions:
    x64, ABM, BMI1, BMI2, ADX,
    SSE, SSE2, SSE3, SSSE3, SSE4.1, SSE4.2,
    AVX, FMA3, AVX2
    AVX512-(F/CD/VL/BW/DQ/IFMA/VBMI)


Target Systems:
    - Intel Cannon Lake and Ice Lake

Recommended For:
    - All Cannon Lake and Ice Lake systems with AVX512.


This binary was tuned on:

    Processor(s)    :   Intel Core i3 8121U
    CPU Frequency   :   2.3 - 3.2 GHz
    Cache Frequency :   2.2 GHz
    Memory          :   8 GB LPDDR4 @ 2666 MHz

    Cores           :   2
    Threads         :   4
    Cache           :   4 MB
    Cache / Threads :   1 MB / thread


--------------------------------------------------------------------------------

Binary: "17-SKX ~ Kotori" (Intel Skylake Purley)


Required Instructions:
    x64, ABM, BMI1, BMI2, ADX,
    SSE, SSE2, SSE3, SSSE3, SSE4.1, SSE4.2,
    AVX, FMA3, AVX2
    AVX512-(F/CD/VL/BW/DQ)


Target Systems:
    - Intel Skylake X and Skylake Purley with 2 x 512-bit FMA.

Recommended For:
    - All Skylake X and Skylake Purley systems with AVX512.


This binary was tuned on:

    Processor(s)    :   Intel Core i9 7940X
    CPU Frequency   :   4.6/4.0/3.6 GHz (all-core non-AVX/AVX/AVX512)
    Cache Frequency :   2.8 GHz
    Memory          :   128 GB DDR4 @ 3466 MHz (16-18-18-38)

    Cores           :   14
    Threads         :   28
    Cache           :   14 MB
    Cache / Threads :   512 KB / thread


--------------------------------------------------------------------------------

Binary: "16-KNL" (Intel Knights Landing Xeon Phi)


Required Instructions:
    x64, ABM, BMI1, BMI2, ADX,
    SSE, SSE2, SSE3, SSSE3, SSE4.1, SSE4.2,
    AVX, FMA3, AVX2
    AVX512-(F/CD)


Target Systems:
    - Intel Knights Landing Xeon Phi

Recommended For:
    - All Intel Xeon Phi with AVX512.


This binary was tuned on:

    This binary is untuned. It uses similar tuning parameters as 17-SKX.


This build is no longer supported as of version 0.7.8.


--------------------------------------------------------------------------------

Binary: "17-ZN1 ~ Yukina" (AMD Zen)


Required Instructions:
    x64, ABM, BMI1, BMI2, ADX,
    SSE, SSE2, SSE3, SSSE3, SSE4.1, SSE4.2,
    AVX, FMA3, AVX2


Target Systems:
    - AMD Zen 1 Summit Ridge

Recommended For:
    - AMD Zen 1 Summit Ridge


This binary was tuned on:

    Processor(s)    :   AMD Ryzen 7 1800X
    Frequency       :   3.8 GHz
    Memory          :   64 GB DDR4 @ 2133 MHz (15-15-15-36)

    Cores           :   8
    Threads         :   16
    Cache           :   16 MB
    Cache / Threads :   1 MB / thread


--------------------------------------------------------------------------------

Binary: "14-BDW ~ Kurumi" (Intel Broadwell)


Required Instructions:
    x64, ABM, BMI1, BMI2, ADX,
    SSE, SSE2, SSE3, SSSE3, SSE4.1, SSE4.2,
    AVX, FMA3, AVX2


Target Systems:
    - Intel Broadwell and Skylake

Recommended For:
    - All Intel Broadwell and Skylake desktop processors.


This binary was tuned on:

    Processor(s)    :   Intel Core i7 6820HK
    Frequency       :   3.20 GHz
    Memory          :   64 GB DDR4 @ 2133 MHz (15-15-15-36)

    Cores           :   4
    Threads         :   8
    Cache           :   8 MB
    Cache / Threads :   1 MB / thread


--------------------------------------------------------------------------------

Binary: "13-HSW ~ Airi" (Intel Haswell)


Required Instructions:
    x64, ABM, BMI1, BMI2,
    SSE, SSE2, SSE3, SSSE3, SSE4.1, SSE4.2,
    AVX, FMA3, AVX2


Target Systems:
    - Intel Haswell

Recommended For:
    - All Intel Haswell processors. Some AMD Carrizo systems may find this
      binary to be faster than the "11-BD1 ~ Miyu" binary.


This binary was tuned on:

    Processor(s)    :   Intel Core i7 5960X
    Frequency       :   4.00 GHz
    Memory          :   64 GB (8 x 8GB) DDR4 @ 2133 MHz (15-15-15-35)

    Cores           :   8
    Threads         :   16
    Cache           :   20 MB
    Cache / Threads :   1 MB / thread


--------------------------------------------------------------------------------

Binary: "11-BD1 ~ Miyu" (AMD Bulldozer)


Required Instructions:
    x64, SSE, SSE2, SSE3, SSSE3, SSE4.1, SSE4.2, AVX, ABM, FMA4, XOP


Target Systems:
    - AMD Piledriver

Recommended For:
    - The AMD Bulldozer family of processors


This binary was tuned on:

    Processor(s)    :   AMD FX-8350
    Frequency       :   4.00 GHz
    Memory          :   32 GB (4 x 8GB) DDR3 @ 1333 MHz (11-11-11-28)

    Cores           :   8 (4 modules)
    Threads         :   8
    Cache           :   8 MB
    Cache / Threads :   1 MB / thread


--------------------------------------------------------------------------------

Binary: "11-SNB ~ Hina" (Intel Sandy Bridge)


Required Instructions:
    x64, SSE, SSE2, SSE3, SSSE3, SSE4.1, SSE4.2, AVX


Target Systems:
    - Intel Sandy Bridge

Recommended For:
    - All Intel Sandy/Ivy Bridge processors


This binary was tuned on:

    Processor(s)    :   Intel Core i7 3630QM
    Frequency       :   3.20 GHz
    Memory          :   8 GB DDR3 @ 1334 MHz (9-9-9-24)

    Cores           :   4
    Threads         :   8
    Cache           :   8 MB
    Cache / Threads :   1 MB / thread


This build will run on any processor supporting AVX instructions. But it is not
recommended for the AMD Bulldozer family due to sub-optimal 256-bit AVX performance.


--------------------------------------------------------------------------------

Binary: "08-NHM ~ Ushio" (Intel Nehalem)


Required Instructions:
    x64, SSE, SSE2, SSE3, SSSE3, SSE4.1


Target Systems:
    - Intel Nehalem

Recommended For:
    - All Intel Nehalem/Westmere processors


This binary was tuned on:

    Processor(s)    :   Intel Core i7 920
    Frequency       :   3.34 GHz (3.50 GHz Turbo Boost)
    QPI             :   6.00 GT/s
    Uncore          :   2.84 GHz
    Memory          :   12 GB (6 x 2GB) DDR3 @ 1335 MHz (9-9-9-25)

    Cores           :   4
    Threads         :   8
    Cache           :   8 MB
    Cache / Threads :   1 MB / thread


This build will also run on Intel Penryn processors. (Intel Core 2 with SSE4.1.)


--------------------------------------------------------------------------------

Binary: "07-PNR ~ Nagisa" (Intel Penryn)


Required Instructions:
    x64, SSE, SSE2, SSE3, SSSE3, SSE4.1


Target Systems:
    - Intel Yorkfield (3 MB cache/thread)

Recommended For:
    - All Intel Core 2 processors with SSE4.1.


This binary was tuned on:

    Processor(s)    :   2 x Intel Xeon X5482 Harpertown
    Frequency       :   3.2 GHz
    FSB             :   1600 MHz
    Memory          :   64 GB (16 x 4GB) DDR2 @ 800 MHz (5-5-5-18)

    Cores           :   8
    Threads         :   8
    Cache           :   24 MB
    Cache / Threads :   3 MB / thread


This build is no longer supported as of version 0.6.1.


--------------------------------------------------------------------------------

Binary: "05-A64 ~ Kasumi" (AMD Athlon 64)


Required Instructions:
    x64, SSE, SSE2, SSE3


Target Systems:
    - AMD K10

Recommended For:
    - All x86-64 processors supporting SSE3 that are not already listed.


This binary was tuned on:

    Processor(s)    :   AMD Phenom X3 720 (4 core unlock)
    Frequency       :   2.80 GHz
    Memory          :   6 GB DDR3 @ 1333 MHz (9-9-9-25)

    Cores           :   4
    Threads         :   4
    Cache           :   6 MB
    Cache / Threads :   1.5 MB / thread


--------------------------------------------------------------------------------

Binary: "04-P4P" (Intel Pentium 4 Prescott)


Required Instructions:
    SSE, SSE2, SSE3


Recommended For:
    - All x86 processors supporting SSE3 that are not already listed.


This binary was tuned on:

    Processor(s)    :   AMD Phenom X3 720 (4 core unlock)
    Frequency       :   2.80 GHz
    Memory          :   6 GB DDR3 @ 1333 MHz (9-9-9-25)

    Cores           :   4
    Threads         :   4
    Cache           :   6 MB
    Cache / Threads :   1.5 MB / thread


--------------------------------------------------------------------------------

Binary: "00-x86" (Legacy x86)


Required Instructions:
    x86/IA-32 since Pentium (BSWAP, CMPXCHG, CPUID, RDTSC, possibly others...)


Recommended For:
    - Legacy x86.


This binary was tuned on:

    Processor(s)    :   AMD Phenom X3 720 (4 core unlock)
    Frequency       :   2.80 GHz
    Memory          :   6 GB DDR3 @ 1333 MHz (9-9-9-25)

    Cores           :   4
    Threads         :   4
    Cache           :   6 MB
    Cache / Threads :   1.5 MB / thread


--------------------------------------------------------------------------------

