The XMP Enhancer Editor is capable of accessing DRAM controller configuration registers of Intel and AMD processors. The idea is to create XMP profiles on the base of the current DRAM timing settings. Unfortunately, not all Intel processors are fully supported due to the lack of technical documentation.

INTEL PROCESSORS:

* 2nd Gen "Sandy Bridge" Desktop & Mobile Intel Core – full support;
* 3rd Gen "Ivy Bridge" Desktop & Mobile Intel Core – full support;
* 3rd Gen Desktop & Server Intel Core and Xeon LGA2011 – full support;
* 4th Gen Desktop & Server Intel Core and Xeon LGA2011-v2 – full support;
* 4th Gen "Haswell" Desktop & Mobile Intel Core – tWR and tWTR timings are not read out;
* 5th Gen Desktop & Server Intel Core and Xeon LGA2011-v3 – tRRD_L is not read. The current DRAM controller frequency is not detected and forced to be displayed at 1067 MHz.
* 6th Gen "Skylake" Desktop & Mobile Intel CPUs with DDR4 DC mode - full support;
* 6th Gen "Skylake" Desktop & Mobile Intel CPUs with DDR3 DC mode - tWR & tWTR are not read out;
* 10th Gen "Ice Lake" Model U/Y CPUs - tRC, tRF2 and tRFC4 are not read out.

AMD PROCESSORS:
 
* 1st Gen AMD Ryzen 1000 Series - full support;
* 2nd Gen AMD Ryzen 2000 Series - full support;
* 3rd Gen AMD Ryzen 3000 Series - full support.