; AST VBIOS Release Notes
;===============================================================================
v.1.14.00: tommyhuang@042225
01.[New]Update version
---------------------------------------------------------------------------------
v.1.13.05: tommyhuang@092524
01.[New]Update version
v.1.13.04: tommyhuang@051324
01.[New]Update version
02.[Bug]Turn on display in the v-sync period.
v.1.13.03: tommyhuang@072423
01.[New]Update version
02.[New] [AST2500] Support AST2500 + IT66121 / IT66122
v.1.13.02: tommyhuang@111622
v.1.13.01: arcsung@081022
v.1.13.00: arcsung@050422
01.[New]Update version
---------------------------------------------------------------------------------
v.1.12.00: arcsung@050121
01.[New]Update version
---------------------------------------------------------------------------------
v.1.11.03: tommyhuang@113020
01.[Bug][AST2600] Fixed display FIFO setting 
v.1.11.02: kuohsiangchou@080720
01.[New][AST2600] Add AST2600 support with ASTDP
02.[New][AST2600] Create BMC load DP FW path and check behavior
---------------------------------------------------------------------------------
v.1.10.01: ycchen@051319
01.[Bug][AST2300] Fixed CVE issue on AST2300
v.1.10.00: ycchen@041519
01.[Bug][DP501] Fixed CVE for DP501
---------------------------------------------------------------------------------
v.1.09.00: ycchen@121418
01.[Bug] Fixed DDC2 SCL & SDA signal align issue
02.[New] Support 1280x960 60Hz
03.[Bug] Initial gamma ramp value to avoid RHEL/CentOS7.5 display abnormal issue 
---------------------------------------------------------------------------------
v.1.08.00: ycchen@050418
01.[Bug][AST2500+DP501] Fixed BMC fw be reset sometimes issue
02.[Bug][AST2500] Modify DRAM settings by H/W request
---------------------------------------------------------------------------------
v.1.07.01: ycchen@010318
01.[Bug] Fixed cause console redirection in VGA only mode
v.1.07.00: ycchen@121217
01.Bump up version only
---------------------------------------------------------------------------------
v.1.06.00: ycchen@112217
01.[Bug][AST2500] disable fast reset after DRAM initial by H/W request
---------------------------------------------------------------------------------
v.1.04.03: ycchen@091117
01.[Bug] [AST2500] Fix stress test failed if alert #EXTRST to low
v.1.04.02: ycchen@082217
01.[Bug] [AST2300/2400/2500] Fix #EXTRST alert to low cause VBIOS failed to POST issue
v.1.04.01: ycchen@072617
01.[Bug] [AST2500+DP501] Fixed AST2500 + DP501 Reboot Stress may cause no dispplay issue
02.[Bug] [AST2500] Fixed incorrect initial settings on some specific platforms
v.1.04.00: ycchen@050417
01.[New] [AST2500] Modify DRAM Settings by H/W request (2017_03_30)
02.[Bug] [AST2500+DP501] Fixed Read EDID Failed Issue
03.[New] [AST2500] Support AST2500 + ITE66121
---------------------------------------------------------------------------------
v.1.03.05: ycchen@010917
01.[Bug] [AST2500] Fixed AST2500 + DP501 cannot display issue
v.1.03.04: ycchen@120916
v.1.03.03: ycchen@101816
01.[New] [AST2500] Support AST2500 + Sil164 (AST2500.DVO)
02.[New] [AST2500] Support AST2500 + DP501 (AST2500.501)
v.1.03.02: ycchen@082316
v.1.03.00: ycchen@070116
01.[Bug] [AST2500] Fixed USB unknown device issue
02.[Bug] [AST2500] Fixed failed to initial DRAM if enable GPIOZ7
03.[New] [AST2400/2500] Support AST2400/2500 + ANX9807
04.[Bug] Fixed system stop at BIOS POST if use 4K2K monitor
05.[New] [DP501] Add S/W Reset for the platform lack of H/W Reset
---------------------------------------------------------------------------------
v.1.02.07: ycchen@032116
01.[New] [AST2300/2400/2500] Use internal delay instead of int15h delay for DRAM initial
v.1.02.06: ycchen@022616
01.[Bug] Fixed resume from pm-suspend failed in VGA only mode on Debian 7.4
02.[Bug] Fixed Screen Abnormal on SLES12 Installation Menu in some case
03.[Bug] [DP501] Modify I2C Timing by request.
04.[Bug] Fixed resume from pm-suspend failed on Ubuntu 14.04
v.1.02.05: ycchen@121515
01.[New] [AST2500] Modify by H/W request (2015_12_12)
v.1.02.04: ycchen@112315
01.[New] Skip to display banner by default
 - VBIOS in .D5 will show and last for 5sec, otherwise will show nothing
v.1.02.03: ycchen@100515
01.[New] [AST2300/2400] New DRAM Setting by H/W request
v.1.02.02: ycchen@082415
01.[New] [AST2400/2300] Support DRAM Auto Sizing in VGA only mode
02.[New] Support 1152x864@75Hz
03.[Bug] [Flash] Fixed 8042 Time Out Issue on Some Platform
v.1.02.01: ycchen@081115
01.[New] Add options for inhibit P2A Access
02.[New] [AST2400/2500] Support 25MHz V-PLL reference Clock
03.[Bug] Fixed pm-suspend resume failed on Debian 7.6.0
---------------------------------------------------------------------------------
v.1.01.05: ycchen@052715
01.[New] use int 15h for delay instead of port 61h, ycchen@042015
02.[Bug] [AST2500] Fixed 1680x1050 display abnormal issue on DELL 2410 monitor
03.[New] [AST2500] Support AST2500 VGA only mode(without BMC)
v.1.01.04: ycchen@041315
01.[Bug] Fixed the miss of 1920x1080 16bpp mode support
02.[Bug] [AST2500] Fixed Threshold Issue for reduced blank mode
03.[New] Support reduced blank mode for 1280x800, 1440x900, 1680x1050 and 1600x900
v.1.01.03: ycchen@040315
01.[New] [AST2500] Remove AST2500A0 VCLK Patch
02.[Bug] [DP501] Fixed cannot display issue with 2-lanes design
03.[Bug] [DP501] Fixed sw reset cause screen blank issue
04.[Bug] [ITE66121] Fixed screen blank issue sometimes
v.1.01.02: ycchen@031815
01.[Bug] Fixed failed to load vesa driver in FreeBSD 10.1, ycchen@021715
02.[Bug] [AST2500] Recover E2M for AST2500A0
v.1.01.01: ycchen@012815
01.[Bug] [DP501] Fixed ARM IRQ8 increase rapidly issue
02.[Bug] Fixed display abnormal on 1366x768 monitor in RHEL6/CentOS6 with basic display video option
v.1.01.00: ycchen@012115
01.[Bug] [Flash] Fixed Flash Utility cannot run properly on some specific platform
02.[Bug] [DP501] Fixed Linux drm driver parsing error if the monitor has EDID extension block
03.[Bug] [AST2500] Disable E2M for AST2500A0
04.[Bug] Remove wide screen mode if iKVM not support wide screen mode
---------------------------------------------------------------------------------
v.1.00.09: ycchen@120414
01.[Bug] [DP501] Avoid noise during mode change, (add delay to 500ms)
v.1.00.08: ycchen@111414
01.[Bug] [DP501] Avoid noise during mode change, ycchen@111314
v.1.00.07: ycchen@091214
01.[New] [AST2400] Enable PCI AER for Windows 2012 WHQL Certificaation
02.[Bug] [ITE66121] Fixed Scratch Incorrect Settings
v.1.00.06: ycchen@080614
v.1.00.05: ycchen@072214
01.[New] Support AST2400+ITE66121
02.[Bug] [DP501] Fixed Win2008R2 BSOD Issue
v.1.00.04: ycchen@071014
01.[Bug] Fixed cannot display logo properly sometimes with ATEN CS-1308/1316 KVM
v.1.00.03: ycchen@063014
01.[Patch] vbetest r6.53 may display abnormal in bank mode
02.[Bug] [DP501] Fixed Install Win2008R2 may casuse Screen Blank
v.1.00.02: ycchen@061414
01.[Patch] [DP501] Patch Screen cannot resume properly if Screen off more than 10 min with AOC i2369 monitor
v.1.00.01: ycchen@060314
01.[Bug] Limit Support Mode to 1024x768 for Non-EDID Monitor
02.[Bug] Fixed video buffer did not clear completely if resolution is above than 1920x1080
03.[Bug] [DP501] Fixed DP501 EDID cannot be parsed properly sometime in VBIOS POST
v.1.00.00: ycchen@052914
01.[New] Support Wide Screen Mode and Parsing for Prefer Mode Timing, ycchen@052914
---------------------------------------------------------------------------------
v.0.99.11: ycchen@050814
01.[Fixed] Fixed Stressed Reboot cause No Display Issue with DP2VGA dongle(chipset:ST,fw:v.1.5) + KVM ATEN CS-1316
v.0.99.10: ycchen@040714
01.[Bug] [DP501] Fixed No Display Issue if BMC reset
02.[Bug] [DP501] Fixed No Display Issue with DP2VGA dongle(chipset:ST,fw:v.1.5 and before) + KVM ATEN CS-1316
03.[Bug] [DP501] Fixed No Display Issue with DP2VGA dongle(chipset:ST,fw:v.1.5 and before) + ASUS VS228H
v.0.99.08: ycchen@021414
01.[Bug] [DP501] Fixed Screen Blank Sometimes and need to re-plug to resume
02.[Bug] [DP501] Improve Display Noisy Issue
v.0.99.07: ycchen@012414
01.[Bug] [DP501] Fixed Screen Blank Sometimes and need to re-plug to resume
v.0.99.06: ycchen@010714
01.[Bug] [DP501] Fixed Screen Blank Sometimes even re-plug DP connector
v.0.99.05: ycchen@122613
01.[Bug] [DP501] Fixed Screen Blank Sometimes even re-plug DP connector
02.[New] [DP501] Modify for Lenovo Ramjet and Renegade SDV
v.0.99.04: ycchen@120613
01.[Bug] [DP501] Fixed EDID cannot be read properly when system reset
v.0.99.03: ycchen@112913
01.[Bug] [DP501] Improve monitor noise when system reboot or shutdown
v.0.99.02: ycchen@112813
01.[Bug] [DP501] Fixed monitor noise when system reboot or shutdown
02.[Bug] [DP501] Screen cannot lose sync. properly for DPMS
v.0.99.01: ycchen@111513
01.[Bug] [DP501] Roll back to hw training due to blank issue still exist by sw training
v.0.99.00: ycchen@111413
01.[Bug] [DP501] Fixed ReadEDID not Stable Issue
02.[Bug] [DP501] Fixed DP Monitor Compatible Issue
---------------------------------------------------------------------------------
v.0.98.03: ycchen@101713
v.0.98.02: ycchen@100913
01.[Bug] Fixed failed to force to VGA
02.[Bug] [ite66121] Fixed failed to disable ASPM
03.[Bug] [DP501] Fixed Screen Sometime Blank Issue
v.0.98.01: ycchen@090413
01.[New] Modify for Scratch Refine for AST2400 + DP501
02.[New] [DP501] Support Read EDID
v.0.98.00: ycchen@061713
01.[New] Support AST2400 + DP501
02.[Bug] [ite66121] Fixed I2C interrupt be trigerred issue
03.[Bug] [ite66121] Fixed ReadEDID not stable issue
---------------------------------------------------------------------------------
v.0.97.06: ycchen@030113
01.[New] Modify for Read EDID Stability (over sample)
02.[New] Support AST2300 + Sil164 (AST2300.DVO)
 - move AST2300 + ITE66121 support to AST2300.ITE
v.0.97.05: ycchen@121212
01.[Bug] Remove Wide Screen Support in VBIOS currently
v.0.97.04: ycchen@112512
01.[New] support vbios that display banner for 5sec
02.[New] Modify for ITE66121 support
03.[Bug] Fixed 800x600 16c mode display abnormal issue (v09700 issue)
v.0.97.03: ycchen@111512
01.[Bug] fixed memory allocation failed issue for some DOS Tools
v.0.97.02: ycchen@110112
01.[Bug] Modify DRAM Setting by H/W request
02.[Bug] Fixed ReadEDID cause system hanged with Avocent KVM
v.0.97.01: ycchen@102912
01.[Bug] Fixed WHCK - PnP Stress Test not Stable Issue
v.0.97.00: ycchen@102612
01.[New] [AST2300/2400] support AST2300/2400 + ITE66121
02.[Bug] Fixed WHCK PnP Stress Test Random Failed Issue
03.[New] Support WXGA modes in VBIOS, including 1280x800, 1440x900, 1680x1050, 1920x1080, 1366x768, 1600x900
04.[Bug] [AST2300/2400] Modify DRAM settings by H/W request
---------------------------------------------------------------------------------
v.0.96.00: ycchen@081412
01.[New] [AST2400] Support AST2400 A0
02.[Bug] [AST2300] Modify DRAM settings for VBIOS coding bug
03.[New] [AST2300/2400] Set DAC source as VGA on POST
04.[New] Modify show logo time to 1sec
---------------------------------------------------------------------------------
v.0.95.01: ycchen@052112
01.[Bug] Fixed iKVM cannot display properly if new VBIOS (v.0.92.00 and after) with older X Windows driver (before v.0.92.00)
02.[New] [AST2300] Modify DRAM settings by H/W request (2012_05_09)
v.0.95.00: ycchen@120224
01.[New] Support AST2400 FPGA
---------------------------------------------------------------------------------
v.0.94.03: ycchen@112311
01.[New] Enable MMIO access by default
02.[Bug] [Flash] Fixed update flash unstable issue on some platform.
v.0.94.02: ycchen@102811
01.[New] [AST2300] Remove the patch for v.0.94.00 #2, Fixed in AMI CRB014 BIOS finally, ycchen@102811
v.0.94.01: ycchen@091611
01.[Bug] [AST2300] Fixed DRAM setting procedure issues
v.0.94.00: ycchen@091311
01.[New] [AST2300] Modify DRAM Settings by H/W Request (07/06/11), ycchen@081011
02.[Bug] [AST2300] Fixed ASPM can't be disabled properly on some specific platform, ycchen@090911
03.[New] [Flash Utility] Modify for General SPI Flash Support
---------------------------------------------------------------------------------
v.0.93.08: ycchen@053111
01.[New] [AST2300] Modify MCLK to 396MHz by H/W request, ycchen@053111
v.0.93.07: ycchen@050911
01.[Bug] Fixed it takes too long time to get EDID from EDID failed monitor
02.[New] Display Bannner include AST1300
v.0.93.04: ycchen@030211
01.[New] [AST2300] Modify for DDR3 2Gb Support
02.[Bug] Fixed Intel iSCSI cursor disappear issue, ycchen@030411
03.[New] [AST2300] Slow CPU/AHB clock in VGA only mode
v.0.93.03: ycchen@021011
01.[New] [AST2300] Modify AST2300 DRAM Timing by H/W Request (020811)
02.[New] [AST2100/2150] Enable AST2100/2150 DRAM Calibration by H/W Request (021411)
v.0.93.02: ycchen@122410
01.[Bug] Fixed INT10 far jmp ptr failed issue
02.[New] Support EFI + VBIOS in one expansion ROM, ycchen@122210
v.0.93.01: ycchen@121410
01.[New] [AST2300] Modify CRT Threshold by H/W Request, ycchen@121410
02.[New] [AST2300] Disable ASPM for VGA Only solution
v.0.93.00: ycchen@121210
01.[New] Modify AST2300 DRAM Timing by H/W Request (121010)
02.[New] Add INT10 Far Call at the offset of 0x06 by DELL's request
---------------------------------------------------------------------------------
v.0.92.02: ycchen@102010
01.[New] Set 800x600 default refresh rate to 60Hz
02.[Bug] Fixed wave form issue on 1280x1024 75Hz and 1280x800 60Hz
03.[New] [AST2300] DRAM type and size selection based on H/W trapping
v.0.92.00: ycchen@080410
01.[New] Add More Mode Info to Scratch for General KVM Need
02.[New] Add for AST2300 VGA only solution
03.[New] Add for AST2300 A1 support
04.[New] Fixed display noise issue during linux kernel reboot (only fixed in AST2300)
---------------------------------------------------------------------------------
v.0.91.0A: ycchen@062210
01.[Bug] Disable E2M for A0 chips issue
v.0.91.09: ycchen@062110
01.[New] Support AST2300 Real chips
02.[New] Disable E2M Read for A0 chips issue
v.0.91.07: ycchen@042110
01.[New] Modify display banner for AST2150/2200
v.0.91.06: ycchen@030410
01.[New] Show Framebuffer size while VBIOS POST
v.0.91.05: ycchen@020310
01.[New] modify for AST2300 FPGA DDR2 & DDR3 support, ycchen@110609
02.[New] Disable PCI-E to M-Bus for AST2300, ycchen@012710
03.[New] Remove Virtual EDID support for other than AST2000, ycchen@020310
v.0.91.00: ycchen@011110
01.[New] Support AST2300 FPGA Board
---------------------------------------------------------------------------------
v.0.90.07: ycchen@102109
01.[BUG] Fix DELL Diag failed issue, ycchen@102109
v.0.90.01: ycchen@082709
01.[Bug] Fixed have chance to get incorrect frame buffer base address if plug two ASPEED's Graphics, ycchen@072709
02.[New] Remove 8bpp VESA modes support above and equal than 1280x1024 due to backwidth issue
03.[New] Add DDR2 512Mx16 266MHz, 1Gx16 266 MHz support for AST2150
v.0.90.00: ycchen@071409
01.[New] remove AST1150 A0 PATCH
---------------------------------------------------------------------------------
v.0.89.07:
01.[New] Modify DRAM timing by H/W request
02.[Bug] Fixed scrolling too slow in EGA mode, ycchen@050809
03.[Bug] Fixed SLES10.2 boot option wait too long issue, ycchen@051109
v.0.89.00: ycchen@121808
01.[New] Add DDR2 1Gx32.266 VBIOS Release for AST2100, ycchen@112608
02.[New] Add patch for AST1150, ycchen@121808
---------------------------------------------------------------------------------
v.0.88.04: ycchen@101408
01.[New] Add AST2100 DVO Support, ycchen@100808
02.[Bug] Fixed code error in SetWriteBank & SetReadBank, ycchen@101408
03.[New] Modify DRAM Reg. Settings by H/W  Request, ycchen@102808
v.0.88.03: ycchen@100208
01.[Bug] Fix DELL RBU cause display blank issue, ycchen@100208
02.[New] Modify for the request of recovery BIOS by QCI
03.[Bug] Modify AST2100 DRAM timing for unstable issue (restore to v.0.88.01)
v.0.88.02: ycchen@090908
01.[New] Bump Version for AST1160
v.0.88.01: ycchen@090208
01.[New] Add AST1100/2050/2100 A2 Chip Identity, ycchen@090108
02.[New] Modify AST1100/2050/2100 DDR2 DRAM Timing by Jason's Request
v.0.88.00: ycchen@082808
01.[BUG] Fixed VGA2 Mirror Display on board solution can't work properly in Windows, ycchen@082708
---------------------------------------------------------------------------------
v.0.87.00: ycchen@072908
01.[PATCH] Patch for AST2100/1100 A2 X-Window Compatible Issue, ycchen@072908
---------------------------------------------------------------------------------
v.0.86.09: ycchen@051208
01.[New] Add DDR2 1Gx16 200MHz support
v.0.86.04: ycchen@032108
01.[Bug] Fixed the background color of edit is incorrect after run cls, ycchen@032108
v.0.86.00: ycchen@012808
01.[New] Modify DRAM settings by H/W (01108)
---------------------------------------------------------------------------------
v.0.85.03: ycchen@010308
01.[New] Modify for DDR 512x16 200MHz settings
v.0.85.02: ycchen@121207
01.[Bug] Fixed DCT/SVGA/INT10 failed issue
02.[New] Modify DDR 512x16 200MHz parameters by H/W  request
v.0.85.01: ycchen@112707
01.[New] Modify DRAM timing by H/W request (11/08/07)
02.[Bug] Fixed display abnormal while new PLL modes change to standard modes, ycchen@112807
03.[New] Remove 1920x1200 for AST1100
04.[New] Modify Display banner for AST1100/2050/2100
05.[Bug] Change 1920x1200x60Hz's polarity to NP
v.0.85.00: ycchen@103107
01.[New] Modify 1920x1200x60Hz to reduced blank mode, ycchen@081307
02.[New] Support ECC
03.[Bug] Fixed PCCheck VGA Palette Test Failed Issue, ycchen@103107
04.[Bug] Fixed Scanline info incorrect in scratch, ycchen@103107
05.[Patch] Patch WDT can't detect mode change properly, ycchen@103107
06.[New] Set Scratch after DRAM Initial
07.[New] Enable Read Cache for AST2100 A1
---------------------------------------------------------------------------------
v.0.84.05: ycchen@072607
01.[New] Disable ReadCache for AST2100 by H/W request
02.[New] Set VGA DRAM Trapping to DRAM Controller, ycchen@072607
v.0.84.04: ycchen@070907
01.[New] Modify DRAM timing for H/W request
v.0.84.03: ycchen@062107
01.[New] Modify DRAM timing to 266MHz
v.0.84.02: ycchen@061507
01.[Bug] Fixed 1920x1200x60Hz can't display
02.[New] Modify DRAM timing by H/W request
v.0.84.01: ycchen@060807
01.[New] Remove Chrontel Setting for real chip
02.[New] Use 512Mb x32 setting as default DRAM type
v.0.84.00: ycchen@060507
01.[New] Support AST2100 A0, ycchen@053107
02.[New] Support 1920x1200x60Hz for AST2100, ycchen@060407
---------------------------------------------------------------------------------
v.0.83.04: ycchen@051507
001.[Bug] Fixed bug check 0xf7 in vista64
v.0.83.03: ycchen@021607
001.[Bug] Fix AST2100 VGA & Video Threshold Issue, ycchen@02160
v.0.83.02: ycchen@020607
001.[Bug] Fix CMDQ & MMIO CMD reorder issue
v.0.83.01: ycchen@011207
001.[New] Modify for AST2100 New IP (0606)
002.[Bug] Fix BCMDiag video memory test failed, ycchen@011206
v.0.83.00: ycchen@120406
001.[New] Support AST2100 FPGA EVB Board
---------------------------------------------------------------------------------
v.0.82.00b: ycchen@092906
001.[New] Initial VGA only if Class Code is VGA Device, ycchen@091506
002.[New] Add the support for VGA initial SOC RTC
003.[New] Add scratch for scan line infor, ycchen@092906
v.0.82.00: ycchen@061406
001. Bump Version Only
---------------------------------------------------------------------------------
v.0.81.01: ycchen@051106
001.[Bug] Fixed save/restore PLL setting incorrect by ycchen@051106
v.0.81.00: ycchen@042406
001.[New] Set MCLK166 as default, ycchen@042406
---------------------------------------------------------------------------------
v.0.80.00: ycchen@031306
001.[BUG] Fixed PCDR/AMIDIAG/BCMDIAG RAMDAC Test too long issue, ycchen@030606
002.[PATCH] Fixed ARC1220 RAID controller display message abnormal issue, ycchen@031006
---------------------------------------------------------------------------------
v.0.63.00: ycchen@020906
001. [Bug] Run PCDR/Video memory test cause KVM crash
---------------------------------------------------------------------------------
v.0.62.00: ycchen@020606
001. [Patch] QCI LCD Monitor display dummy under the bottom of the screen
---------------------------------------------------------------------------------
v.0.61.00: ycchen@011106
001.[Bug] fixed VRS/VRE incorrect issue, ycchen@122805
002.[New] 32k VBIOS as default
003.[New] Modify for product description
004.[New] Support 16/32 DRAM in one VBIOS
005.[Bug] Can't Set VESA Mode: 1280x1024x32bpp, ycchen@010606
006.[Bug] 640x480x72Hz Border issue
007.[Bug] Modify for low-reslution timing, ycchen@011005
008.[Bug] fixed AMIDIAG\VESA memory test failed issue, ycchen@011206
009.[Bug] Modify for CRTC timing for STD. mods, ycchen@011206
---------------------------------------------------------------------------------
v.0.60.00: ycchen@12202005, first release for A1
001.[New] Modify for A1 support
002.[New] Integrate LFB/UMA VBIOS into one (ASTVBIOS.ROM)
---------------------------------------------------------------------------------
v.0.52.00: ycchen@11042005
1. [New] Change Device to 0x1A03
---------------------------------------------------------------------------------
v.0.51.00: ycchen@10252005
1. [Bug] Fixed ReadHat9 Install Shell Display Abnormal Issue
2. [New] Modify for DRAM init status check in UMA mode
3. [New] Support Customizded DRAM timing in binary level
4. [New] Support Virtual EDID
5. [Bug] Install RHEL hanged before enter into X-Window on Operon
6. [Bug] Modify for CRTC Timing for standrad mode & low resolution mode
7. [New] Add Support VESA Mode: 1280x1204, 1600x1200, 320x240, 400x300 and 512x384
---------------------------------------------------------------------------------
v.0.50.00: ycchen@10122005
1. The first release for A0
