Marvell AQC107 FW Package

File
--------
DASH Linux TOOL
-AqDashConfig
-AqDashAgent

DASH Windows TOOL
-AqDashConfig-v0.32:Dash config tool
-AqDashAgent-v0.32:Dash agent

atlflashupdate_1.8.0_4.2.46dash.tar:FW update package Linux version
atlflashupdate_1.8.0_4.2.46dash.zip:FW Update package Windows version
How to use self-signed certificates for HTTPS communication.docx: Describes how to create certificates files(crt file and key file)

FW version
----------
4.2.46

What's new
-----------
Fixed changing operating-system state to "Quiesce" if host OS is in sleep or being restarted.
Stopped Dhcp release in case of link down when static ip is configured in exclusive mode. 

FW Update by manually
---------------------
1 unzip atlflashupdate package
2.1.1 [Windows] run CMD as Administrator
2.1.2 cd ...\atlflashupdate_x.x.x_x.x.xxdash
2.1.3 atlflashupdate.exe -s
2.2.1 [Linux] tar -zxvf xxxx.tar.gz
2.2.2 chomod 777 atlflashupdate
2.2.3 ./atlflashupdate -s -a "device_name", device name can check with command "ifconfig"

Note:only support PCI\VEN_1D6A&DEV_07B1&SUBSYS_104617AA

FW Update by DASH
-----------------
please follow AMC Console or Dashcli User guide to update FW via DASH

Note: if use Dash to update FW, don't unzip the atlflashupdate_x.x.x_x.x.xxdash


Enable DASH
-------------
1 run CMD or Powershell as Administrator
2.1 AqDashConfig.exe exclusive <user> <password> <crt file> <key file> --mac <DASH MAC address> --ip <DASH IP address> --device <Name>
2.2 AqDashConfig.exe shared <user> <password> <crt file> <key file> --device <Name>
3.1 AqDashAgent.exe install

Note:If system have two or more AQC107/AQN107, --device <Name> is must, can check in device manager. 
Only onboard AQC107 support DASH.
In exclusive mode, DASH MAC address must different tartget's MAC address, DASH IP address have same rule.


DISABLE DASH
-------------
1 run CMD or Powershell as Administrator
2 AqDashConfig.exe disable
3 AqDashAgent.exe uninstall


TOOLS_VERSION=1.8.0

