#==========================================
# BMC firmware update tool 
# version 1.0.1
#==========================================

windows:
	remote:
		FWUpdate_Win.bat [IP] [Username] [password]

	local:
		FWUpdate_Win.bat -local [Username] [password]
		ps. AMI Remote RNDIS based Device driver is needed

Linux:
	remote:
		./FWUpdate_Linux.sh [IP] [Username] [password]

	local:
		./FWUpdate_Linux.sh -local [Username] [password]


* Note : If can not creat IPMI session when update firmware that need to install libssl-dev(openssl crypto library)
