;===============================================================================
; ASPEED Graphics UEFI Driver Release Notes
;===============================================================================
v.1.14.00: tommyhuang@042225
01.[New]Update version
02.[New][AST2700 A1] Add AST2700 A1 binary support.
03.[Del][AST2700 A0] Remove AST2700 A0 DCSCM binary.
---------------------------------------------------------------------------------
v.1.13.05: tommyhuang@110824
01.[Bug][AST2500 / AST2600] Add EDID divid value check.
02.[New][AST2500 / AST2600] Turn off hardware cursor.
03.[New][AST2500 / AST2600] Update build server name.
v.1.13.04: tommyhuang@051324
01.[Bug][AST2600] Turn on display in the V-sync avoid garbage flick issue.
02.[Bug][AST2500 / AST2600] Check the EDID valid by EDID header checked.
03.[Del][AST2500 / AST2600] Remove 800x600@56 form UEFI GOP.
04.[Del][AST2500] Support AST2500 + IT66121 / IT66122
v.1.13.03: tommyhuang@072423
01.[Bug][AST2600][ARM] Fixed report framebuffer base behavior.
02.[Del][AST2600][X64] Remove CSM-auto binary
03.[New][AST2500] Support AST2500 + IT66121 / IT66122
v.1.13.02: tommyhuang@111622
01.[New] Add aarch64 binry release.
02.[New][AST2600] Add CSM-auto binary for X64
03.[New][AST2600] Add VGA only flag
v.1.13.01: arcsung@081022
01.[New][AST2600] disable CSM-auto on aarch64.
v.1.13.00: arcsung@050422
01.[New][AST2600] System booting with VBIOS installed OS as CSM-auto.
---------------------------------------------------------------------------------
v.1.12.00: arcsung@050121
01.[New][AST2600] Check BMC init, or skip GOP.
02.[New][AST2600] Add reserver 4M feature on AST2600.
---------------------------------------------------------------------------------
v.1.11.03: tommyhuang@113020
01.[Bug][AST2600] Fixed display FIFO setting 
v.1.11.02: kuohsiangchou@080720
01.[New][AST2600] Add AST2600 support with ASTDP
02.[New][AST2600] Create BMC load DP FW path and check behavior
---------------------------------------------------------------------------------
v.1.10.01: ycchen@051319
v.1.10.00: ycchen@041219
01.[Bug][AARCH64] Fixed hanged issue if disable P2A
02.[Bug] Fixed "reconnect -r" failed issue
03.[Bug][DP501] Fixed CVE for DP501 
-------------------------------------------------------------------------------  
v.1.09.00: ycchen@121318
01.[Bug] Initial gamma lut to fix display abnormal issue on RHEL/CentOS 7.5
-------------------------------------------------------------------------------
v.1.08.00: ycchen@050418
01.[Bug][AST2500+DP501] Fixed BMC fw be reset sometimes issue
02.[Bug][AST2500] Modify DRAM settings by H/W request
03.[New] Migrate to EDK2-UDK2018
-------------------------------------------------------------------------------
v.1.07.01: ycchen@010318
01.[Bug] Fixed cause console redirection in VGA only mode
v.1.07.00: ycchen@121217
01.[Bug] Fixed "reconnect -r" failed on Intel's platform
-------------------------------------------------------------------------------
v.1.06.00: ycchen@112217
01.[Bug] Fixed MaxMode is zero if the Monitor's EDID lack of detailed timing
02.[Bug][AST2500] disable fast reset after DRAM initial by H/W request
---------------------------------------------------------------------------------
v.1.04.03: ycchen@091117
01.[Bug] [AST2500] Fix stress test failed if alert #EXTRST to low
v.1.04.02: ycchen@082217
v.1.04.01: ycchen@072617
01.[Bug] [AST2500+DP501] Fixed AST2500 + DP501 Reboot Stress may cause no dispplay issue
v.1.04.00: ycchen@050417
01.[New] [AST2500] Modify DRAM Settings by H/W request (2017_03_30)
02.[Bug] [AST2500+DP501] Fixed Read EDID Failed Issue
03.[New] [AST2500] Support AST2500 + ITE66121
---------------------------------------------------------------------------------
v.1.03.05: ycchen@010917
01.[Bug] [AST2500] Fixed AST2500 + DP501 cannot display issue
v.1.03.04: ycchen@120916
01.[Bug] [GOP] Fixed "reconnect -r" failed issue
02.[Bug] [GOP] Fixed Scrolling Screen Abormal if disable P2A
v.1.03.03: ycchen@101816
01.[New] [AST2500] Support AST2500 + Sil164 (AST2500.DVO)
02.[New] [AST2500] Support AST2500 + DP501 (AST2500.501)
v.1.03.02: ycchen@082316
01.[Bug] Fixed display garbage issue for early display
v.1.03.00: ycchen@070116
01.[Bug] [AST2500] Fixed USB unknown device issue
02.[Bug] [AST2500] Fixed failed to initial DRAM if enable GPIOZ7
03.[New] [AST2400/2500] Support AST2400/2500 + ANX9807
04.[New] [DP501] Add S/W Reset for the platform lack of H/W Reset
---------------------------------------------------------------------------------
v.1.02.07: ycchen@032316
v.1.02.06: ycchen@022616
01.[Bug] [DP501] Modify I2C Timing by request.
v.1.02.05: ycchen@121515
01.[New] [AST2500] Modify by H/W request (2015_12_12)
02.[Bug] [ITE66121] Fixed Screen Blank Sometimes
v.1.02.04: ycchen@112315
v.1.02.03: ycchen@100515
01.[New] [AST2300/2400] New DRAM Setting by H/W request
02.[New] Flash tool in UEFI Shell
v.1.02.02: ycchen@082415
01.[New] [AST2400/2300] Support DRAM Auto Sizing in VGA only mode
v.1.02.01: ycchen@072715
01.[New] Add options for inhibit P2A Access
02.[New] [AST2400/2500] Support 25MHz V-PLL reference Clock
---------------------------------------------------------------------------------
v.1.01.05: ycchen@052715
01.[Bug] [AST2500] Fixed 1680x1050 display abnormal issue on DELL 2410 monitor
02.[New] [AST2500] Support AST2500 VGA only mode(without BMC)
v.1.01.04: ycchen@041315
01.[Bug] [AST2500] Fixed Threshold Issue for reduced blank mode
02.[Bug] Fixed flash utility cannot backup uefi gop image properly
03.[New] Support reducded blank mode for 1280x800, 1440x900, 1680x1050 and 1600x900
v.1.01.03: ycchen@040315
01.[New] [AST2500] Remove AST2500A0 VCLK Patch
02.[Bug] [DP501] Fixed cannot display issue with 2-lanes design
03.[Bug] [DP501] Fixed sw reset cause screen blank issue
04.[Bug] [ITE66121] Fixed screen blank issue sometimes
v.1.01.02: ycchen@031815
01.[Bug] Fixed Failed to Install Driver on Windows2012
v.1.01.01: ycchen@012815
01.[Bug] [DP501] Fixed ARM IRQ8 increase rapidly issue
v.1.01.00: ycchen@012215
01.[New] Support AST2500 and AST2400+ITE66121
02.[Bug] [DP501] Fixed Linux drm driver parsing error if the monitor has EDID extension block
03.[Bug] Remove wide screen mode if iKVM not support wide screen mode
-------------------------------------------------------------------------------
v.1.00.10: ycchen@121914
01.[Bug] Fixed Failed to Load on Intel UEFI BIOS, ycchen@121914
v.1.00.09: ycchen@120414
v.1.00.08: ycchen@120314
01.[Bug] Fixed 1366x768 display abnormal on Windows 2012 Installation
v.1.00.07: ycchen@091214
01.[New] [AST2400] Enable PCI AER for Windows 2012 WHQL Certificaation
02.[Bug] Fixed "CR has Bad Signature" with newer AMI CSM Modules
03.[Bug] [ITE66121] Fixed Scratch Incorrect Settings
v.1.00.06: ycchen@080514
01[Bug] Fixed 1366x768 cannot display properly
v.1.00.05: ycchen@072314
01.[New] Support AST2400+ITE66121
02.[Bug] [DP501] Fixed Win2008R2 BSOD Issue
v.1.00.04: ycchen@071014
v.1.00.03: ycchen@063014
01.[Bug] [DP501] Fixed Install Win2008R2 may casuse Screen Blank
v.1.00.02: ycchen@061414
01.[Patch] [DP501] Patch Screen cannot resume properly if Screen off more than 10 min with AOC i2369 monitor
v.1.00.01: ycchen@060514
v.1.00.00: ycchen@052914
01.[New] Support Wide Screen Mode and Parsing for Prefer Mode Timing, ycchen@052914
---------------------------------------------------------------------------------
v.0.99.12: ycchen@051314
01.[Fixed] Fixed Screen No Display Issue if attached non-EDID monitor with v.0.99.11 GOP driver
v.0.99.11: ycchen@050814
01.[Fixed] Fixed Stressed Reboot cause No Display Issue with DP2VGA dongle(chipset:ST,fw:v.1.5) + KVM ATEN CS-1316
02.[Fixed] Fixed Monitor "Out of Screen" Issue if Install RHEL6.4 in UEFI Mode
v.0.99.10: ycchen@040714
01.[Bug] [DP501] Fixed No Display Issue if BMC reset
02.[Bug] [DP501] Fixed No Display Issue with DP2VGA dongle(chipset:ST,fw:v.1.5 and before) + KVM ATEN CS-1316
03.[Bug] [DP501] Fixed No Display Issue with DP2VGA dongle(chipset:ST,fw:v.1.5 and before) + ASUS VS228H
v.0.99.08: ycchen@021714
v.0.99.07: ycchen@012414
01.[Bug] [DP501] Fixed Screen Blank Sometimes and need to re-plug to resume
v.0.99.06: ycchen@010714
01.[Bug] [DP501] Fixed Screen Blank Sometimes even re-plug DP connector
v.0.99.05: ycchen@122613
01.[Bug] [DP501] Fixed Screen Blank Sometimes even re-plug DP connector
02.[New] [DP501] Modify for Lenovo Ramjet and Renegade SDV
v.0.99.04: ycchen@120613
01.[Bug] [DP501] Fixed EDID cannot be read properly when system reset
v.0.99.03: ycchen@112913
01.[Bug] [DP501] Fixed monitor noise when system reboot or shutdown
v.0.99.01: ycchen@112113
01.[Bug] [DP501] Fixed DP Monitor Compatible Issue
v.0.99.00: ycchen@111113
01.[New] [DP501] Direct Access EDID
-------------------------------------------------------------------------------
v.0.98.04: ycchen@110113
01.[Bug] Fixed AST2400 + DP501 cannot display issue
v.0.98.01: ycchen@100813
01.[New] Support AST2400 + DP501
02.[Bug] Fixed Driver Version not show correctly issue
03.[Bug] Fixed Win2008 Installation Screen Abnormal with UEFI + Legacy option ROM
04.[New] use MMIO instead
-------------------------------------------------------------------------------
v.0.97.06: ycchen@032013
01.[New] Support AST2300/2400 + DVO, AST2300 + ITE66121
02.[Bug] Modify for Read EDID un-stable issue
v.0.97.05: ycchen@121812
01.Remove Wide Screen Support
v.0.97.04: ycchen@112912
01.[AST2300/2400] [Bug] Modify for DRAM Settings by H/W Request
02.[New] Support Wide Screen Modes
03.[Bug] [AST1100/2050/2100/2150/2200] Fixed Display Abnormal Issue in VGA only mode
04.[New] [AST2300] Disable ASPM in GOP driver
05.[New] [AST2300/2400] Support AST2300/2400 + ITE66121
-------------------------------------------------------------------------------
v.0.96.00: ycchen@081412
01.[Bug] Fixed failed to install Win8
02.[New] [AST24000] Support AST2400
03.[New] [AST2300/2400] Modify DRAM Setting for H/W Request (2012_5_9)
04.[New] [AST2300/2400] Set VGA as DAC output
v.0.93.08: ycchen@053111
01.[New] [AST2300] Modify MCLK to 396MHz by H/W request
v.0.93.07: ycchen@050911
01.[Bug] Fixed it takes too long time to get EDID from EDID failed monitor
v.0.93.04: ycchen@030411
01.[New] [AST2300] Modify for DDR3 2Gb Support
02.[New] [AST2300] Slow Down CPU/AHB clock in VGA only mode
v.0.93.03: ycchen@021511
01.[New] [AST2300] Modify AST2300 DRAM Timing by H/W Request (020811)
02.[New] [AST2100/2150] Enable AST2100/2150 DRAM Calibration by H/W Request (021411)
v.0.93.02: ycchen@122410
01.First Release
