AMD Software Release Notes ver. 5.05.23.438

Package Contents and Compatible Operating Systems

This Software package contains various independent drivers (Column 1) designed to support the following OS (Column 3). Operating System support may vary depending on your specific AMD product

Driver Name	Supported Version	Supported OS	
AMD I2C Driver for Server	1.2.0.120	Windows® Azure Stack HCI v2/21H2	
	1.2.0.120	Windows® Server 2022	
	1.2.0.120	Windows® Server 2019	
	1.2.0.120	Windows® 11	
	1.2.0.120	Windows® 10	
	1.2.0.120	Windows® Azure Stack HCI v3/22H2	
AMD UART Driver for Server	1.2.0.106	Windows® Azure Stack HCI v2/21H2	
	1.2.0.106	Windows® Server 2022	
	1.2.0.106	Windows® Server 2019	
	1.2.0.106	Windows® 11	
	1.2.0.106	Windows® 10	
	1.2.0.106	Windows® Azure Stack HCI v3/22H2	
AMD GPIO2 Driver for Server	2.2.0.126	Windows® Azure Stack HCI v2/21H2	
	2.2.0.126	Windows® Server 2022	
	2.2.0.126	Windows® Server 2019	
	2.2.0.126	Windows® 11	
	2.2.0.126	Windows® 10	
	2.2.0.126	Windows® Azure Stack HCI v3/22H2	
AMD PSP Driver for Server	4.10.0.3	Windows® Azure Stack HCI v2/21H2	
	4.10.0.3	Windows® Server 2022	
	4.10.0.3	Windows® Server 2019	
	4.10.0.3	Windows® 11	
	4.10.0.3	Windows® 10	
	4.10.0.3	Windows® Azure Stack HCI v3/22H2	
AMD EPYC DRTM Boot Driver	1.10.3.0	Windows® Azure Stack HCI v2/21H2	
AMD Interface	2.0.0.10	Windows® Azure Stack HCI v2/21H2	
	2.0.0.10	Windows® Server 2022	
	2.0.0.10	Windows® Server 2019	
	2.0.0.10	Windows® 11	
	2.0.0.10	Windows® 10	
	2.0.0.10	Windows® Azure Stack HCI v3/22H2	
AMD EPYC DRTM Boot Driver	1.10.3.0	Windows® Azure Stack HCI v3/22H2	
AMD EPYC DRTM Boot Driver	1.10.3.0	Windows® Server 2022	

Known Issues:

·	NA

Installation of Software:

·	Unzip the compressed package.
·	Double click on executable named AMD_Chipset_Drivers_<VersionNumber>.exe.
·	Provide administrative privilege if prompted, by clicking ‘YES’ in the UAC prompt.
·	By default, the executable extracts files under "C:\AMD\AMD_Chipset_Drivers" and continues with installation.

Uninstallation of Software:

·	Once installation completes successfully, invoke maintenance mode of installer through either of the below:
·	Click ‘Uninstall/Change’ after selecting ‘AMD Chipset Drivers’ entry in control panel.
·	Double-click on the installation executable to run it in maintenance mode.

·	after above step, user will get options of ‘Modify’ and ‘Remove’:
·	Modify: List out all drivers available for that platform with their current state in the system.
·	Driver names with cross mark indicates that, the driver component is not installed. Driver component without cross mark indicates that, the driver is installed on the system.
·	Based on the need, a user can choose either of the following:
·	Mark an already installed driver with cross, so that it will be removed from the system on completion of maintenance mode process.
·	Unmark a driver so that it gets deployed on the system.
This choice can be made to any number of drivers in the list and proceed with Modify option.

·	Remove: A single click which removes all uninstall-able drivers deployed by AMD_Chipset_Drivers_<VersionNumber>.exe from the system.

Installation using the Command Line Interface

To perform an unattended installation of the Software using the Command Line Interface, please follow the below steps

·	Unzip Package:
·	Release Notes 
·	’AMD_Chipset_Drivers_<VersionNumber>.exe’

·	Invoke ’AMD_Chipset_Drivers_<VersionNumber>.exe’ on elevated command prompt with below options:

Silent deployment scenarios	Commands to be used	
Silent Install	START /WAIT "" <path to executable with exe name> /S 	
Silent Uninstall	START /WAIT "" <path to executable with exe name> /S /EXPRESSUNINSTALL=1	
Custom Silent Install	START /WAIT "" <path to executable with exe name> /S /CUSTOMINSTALL="<feature name/names assigned to the drivers that are to be installed separated by comma>"	
Custom Silent Uninstall	START /WAIT "" <path to executable with exe name> /S /CUSTOMUNINSTALL="<feature name/names assigned to the drivers that are to be uninstalled separated by comma>"	
Silent install switch which will NOT show reboot pop-up and suppress auto reboot even if reboot is detected.	START /WAIT "" <path to executable with exe name> /S /REBOOTPROMPT=S /REBOOT=ReallySuppress	
Silent install switch which will NOT show reboot pop-up but automatically reboots the system as and when it is detected without any intimation to user.	START /WAIT "" <path to executable with exe name> /S /REBOOTPROMPT=S	
Complete uninstall which will NOT show reboot pop-up and suppress auto reboot even if reboot is detected	START /WAIT "" <path to executable with exe name> /S /EXPRESSUNINSTALL=1 /REBOOTPROMPT=S /REBOOT=ReallySuppress

Installation using the Power Shell Interface

To perform an unattended installation of the Software using the Command Line Interface, please follow the below steps

·	Unzip Package and copy the executable to System Under Test:
·	Release Notes 
·	’AMD_Chipset_Drivers_<VersionNumber>.exe’

·	Invoke ’AMD_Chipset_Drivers_<VersionNumber>.exe’ on elevated Power Shell Interface with below options:

Silent deployment scenarios	Commands to be used	
Silent Install	Start-Process -NoNewWindow -FilePath "<path to executable with exe name>” -ArgumentList “/S” 	
Silent Uninstall	Start-Process -NoNewWindow -FilePath "<path to executable with exe name>” -ArgumentList “/S /EXPRESSUNINSTALL=1”	
Custom Silent Install	Start-Process -NoNewWindow -FilePath "<path to executable with exe name>” -ArgumentList “/S /CUSTOMINSTALL=<feature name/names assigned to the drivers that are to be installed separated by comma>”	
Custom Silent Uninstall	Start-Process -NoNewWindow -FilePath "<path to executable with exe name>” -ArgumentList “/S /CUSTOMUNINSTALL=<feature name/names assigned to the drivers that are to be uninstalled separated by comma>”	
Silent install switch which will NOT show reboot pop-up and suppress auto reboot even if reboot is detected.	Start-Process -NoNewWindow -FilePath "<path to executable with exe name>” -ArgumentList “/S /REBOOTPROMPT=S /REBOOT=ReallySuppress”	
Silent install switch which will NOT show reboot pop-up but automatically reboots the system as and when it is detected without any intimation to user.	Start-Process -NoNewWindow -FilePath "<path to executable with exe name>” -ArgumentList “/S /REBOOTPROMPT=S”	
Complete uninstall which will NOT show reboot pop-up and suppress auto reboot even if reboot is detected	Start-Process -NoNewWindow -FilePath "<path to executable with exe name>” -ArgumentList “/S /EXPRESSUNINSTALL=1 /REBOOTPROMPT=S /REBOOT=ReallySuppress”

·	Please find the feature name/names assigned to respective drivers as below:
                
Driver Name	Corresponding feature name to be passed in command line	
AMD CCP Driver   	CCP	
AMDGPIO2 for Server	GPIO2_SVR	
AMDI2C for Server	I2C_SVR	
AMD PCI Device Driver for Server	PCI_SVR	
AMD PSP for Server	PSP_SVR	
AMD SMBUS Driver	SMBUS	
AMDUART for Server	UART_SVR	
AMD IOV for server	IOV_SVR	
AMD XHCI Reg driver	XHCIREG	
AMD INTERFACE Driver	INT_SVR	
AMD EPYC DRTM Boot Driver	DRTM_SVR	

© 2023 Advanced Micro Devices, Inc.  All Rights Reserved.
WARNING: AMD processors, including chipsets, CPUs, APUs and GPUs (collectively and individually “AMD processor”), are intended to be operated only within their associated specifications and factory settings. Operating your AMD processor outside of official AMD specifications or outside of factory settings, including but not limited to the conducting of overclocking (including use of this overclocking software, even if such software has been directly or indirectly provided by AMD or an entity otherwise affiliated in any way with AMD), may damage your processor, affect the operation of your processor or the security features therein and/or lead to other problems, including but not limited to damage to your system components (including your motherboard and components thereon (e.g., memory)), system instabilities (e.g., data loss and corrupted images), reduction in system performance, shortened processor, system component and/or system life, and in extreme cases, total system failure. It is recommended that you save any important data before using the tool.  AMD does not provide support or service for issues or damages related to use of an AMD processor outside of official AMD specifications or outside of factory settings. You may also not receive support or service from your board or system manufacturer. Please make sure you have saved all important data before using this overclocking software. DAMAGES CAUSED BY USE OF YOUR AMD PROCESSOR OUTSIDE OF OFFICIAL AMD SPECIFICATIONS OR OUTSIDE OF FACTORY SETTINGS ARE NOT COVERED UNDER ANY AMD PRODUCT WARRANTY AND MAY NOT BE COVERED BY YOUR BOARD OR SYSTEM MANUFACTURER’S WARRANTY.