Copyright 2025 ADVANCED MICRO DEVICES, INC. All Rights Reserved. 

AMD RAID controller Driver distribution list
Revision: 9.3.3.00245
Built date: 06/18/2025
OS: 
•	Windows10 x64
•	Windows11 x64 (21H2, 22H2, 23H2 & 24H2)
Supported Products:
•	Workstation 	: AMD Ryzen™ Threadripper™ 9000, 7000, 5000 Series.
•	Chipsets 	: WRX90, TRX50, WRX80, TRX40 Series.                  

AMD-RAID binary file name:
	Windows UWP:
•	RAIDXpert2 UWP application
•	RAIDXpert2 Security Certificate
•	RAIDXpert2 Personal Information Exchange

RAIDXPert2 Application:
•	RAIDXpert2-Management-Suite.exe
	
Known issues.
•	The RAIDXpert2 application may freeze or become unresponsive after an array transformation or reconnecting a removed NVMe. 

Revision History
•	9.3.3.00245
-	Fix LED blink pattern for disk identify and rebuild.
•	9.3.3.00238
-	Updated User guide to v3.31.
-	Fix for access user guide shortcut.
•	9.3.3.00218
-	Resolved UI navigation issue on EULA window.
•	9.3.3.00187
-	Added caution message to remove associated arrays with NVMe Front Bay before performing prepare to removal of devices.
•	9.3.3.00144
-	EULA appears at the first launch of Raidxpert2 GUI application.
•	9.3.3.00117
-	Enhanced led blink command as part of prepare to remove device.
-	The application now uses QT6 Framework.
•	9.3.3.00097
-	Enabled RAID5 support for new programs.
-	Fixed raidxpert2 application signing compliance.
-	Updated User guide to v3.30.
•	9.3.3.00068
-	Fixed prepare to removal of Legacy arrays.
-	Fixed appropriate log message when NVMe are removed from the system.
-	Blocked removal of array when IO is in progress.
-	Changed text color when arrays are in hide state.
•	9.3.3.00012
-	Added partition column to the radm.exe to map partition label.
•	9.3.3.00006
-	Created a new branch to support new OS and other RAID features.